,H Height##LENGTH##FRACTIONAL FEET,C##LENGTH##FRACTIONAL FEET,URL Product Performance Data##OTHER##,Blade Quantity##OTHER##,Air Terminal Material##OTHER##,Optional Center Divider##OTHER##,D##LENGTH##FRACTIONAL FEET,Air Terminal Static Pressure##HVAC_PRESSURE##INCHES_OF_WATER,W Width##LENGTH##FRACTIONAL FEET,Keynote##OTHER##,Duct Height##LENGTH##FRACTIONAL FEET,Assembly Code##OTHER##,URL Product Data Sheet##OTHER##,Actual Supply Air Flow##HVAC_AIR_FLOW##CUBIC_FEET_PER_MINUTE,Content Developer Contact##OTHER##,A##LENGTH##FRACTIONAL FEET,Duct Width##LENGTH##FRACTIONAL FEET
35" x12",1.161,0.506,http://www.kees.com/pdf/pdssdl.pdf,6,Stainless Steel,0,0.233,0,3.156,KEES,1.016,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.573,2.99
15" x10",0.995,0.511,http://www.kees.com/pdf/pdssdl.pdf,2,Stainless Steel,0,0.183,0,1.49,KEES,0.849,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.49,1.323
60" x10",0.995,0.511,http://www.kees.com/pdf/pdssdl.pdf,11,Stainless Steel,0,0.183,0,5.24,KEES,0.849,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.49,5.073
12" x 6",0.734,0.306,http://www.kees.com/pdf/pdssdl.pdf,3,Stainless Steel,0,0.093,0,1.224,KEES,0.536,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.281,1.073
15" x15",1.417,0.683,http://www.kees.com/pdf/pdssdl.pdf,2,Stainless Steel,0,0.277,0,1.49,KEES,1.271,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.818,1.323
30" x12",1.161,0.506,http://www.kees.com/pdf/pdssdl.pdf,5,Stainless Steel,0,0.233,0,2.74,KEES,1.016,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.573,2.573
20" x12",1.161,0.506,http://www.kees.com/pdf/pdssdl.pdf,3,Stainless Steel,0,0.233,0,1.906,KEES,1.016,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.573,1.74
60" x 6",0.734,0.306,http://www.kees.com/pdf/pdssdl.pdf,19,Stainless Steel,0,0.093,0,5.24,KEES,0.536,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.281,5.073
50" x10",0.995,0.511,http://www.kees.com/pdf/pdssdl.pdf,9,Stainless Steel,0,0.183,0,4.406,KEES,0.849,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.49,4.24
20" x10",0.995,0.511,http://www.kees.com/pdf/pdssdl.pdf,3,Stainless Steel,0,0.183,0,1.906,KEES,0.849,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.49,1.74
50" x12",1.161,0.506,http://www.kees.com/pdf/pdssdl.pdf,9,Stainless Steel,0,0.233,0,4.406,KEES,1.016,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.573,4.24
60" x15",1.417,0.683,http://www.kees.com/pdf/pdssdl.pdf,11,Stainless Steel,0,0.277,0,5.24,KEES,1.271,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.818,5.073
40" x15",1.417,0.683,http://www.kees.com/pdf/pdssdl.pdf,7,Stainless Steel,0,0.277,0,3.573,KEES,1.271,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.818,3.406
70" x10",0.995,0.511,http://www.kees.com/pdf/pdssdl.pdf,13,Stainless Steel,0,0.183,0,6.073,KEES,0.849,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.49,5.906
25" x12",1.161,0.506,http://www.kees.com/pdf/pdssdl.pdf,4,Stainless Steel,0,0.233,0,2.323,KEES,1.016,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.573,2.156
30" x10",0.995,0.511,http://www.kees.com/pdf/pdssdl.pdf,5,Stainless Steel,0,0.183,0,2.74,KEES,0.849,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.49,2.573
30" x15",1.417,0.683,http://www.kees.com/pdf/pdssdl.pdf,5,Stainless Steel,0,0.277,0,2.74,KEES,1.271,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.818,2.573
24" x 6",0.734,0.306,http://www.kees.com/pdf/pdssdl.pdf,7,Stainless Steel,0,0.093,0,2.24,KEES,0.536,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.281,2.073
40" x12",1.161,0.506,http://www.kees.com/pdf/pdssdl.pdf,7,Stainless Steel,0,0.233,0,3.573,KEES,1.016,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.573,3.406
20" x15",1.417,0.683,http://www.kees.com/pdf/pdssdl.pdf,3,Stainless Steel,0,0.277,0,1.906,KEES,1.271,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.818,1.74
25" x10",0.995,0.511,http://www.kees.com/pdf/pdssdl.pdf,4,Stainless Steel,0,0.183,0,2.323,KEES,0.849,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.49,2.156
35" x10",0.995,0.511,http://www.kees.com/pdf/pdssdl.pdf,6,Stainless Steel,0,0.183,0,3.156,KEES,0.849,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.49,2.99
30" x 6",0.734,0.306,http://www.kees.com/pdf/pdssdl.pdf,9,Stainless Steel,0,0.093,0,2.74,KEES,0.536,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.281,2.573
25" x15",1.417,0.683,http://www.kees.com/pdf/pdssdl.pdf,4,Stainless Steel,0,0.277,0,2.323,KEES,1.271,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.818,2.156
15" x 6",0.734,0.306,http://www.kees.com/pdf/pdssdl.pdf,4,Stainless Steel,0,0.093,0,1.49,KEES,0.536,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.281,1.323
15" x12",1.161,0.506,http://www.kees.com/pdf/pdssdl.pdf,2,Stainless Steel,0,0.233,0,1.49,KEES,1.016,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.573,1.323
18" x 6",0.734,0.306,http://www.kees.com/pdf/pdssdl.pdf,5,Stainless Steel,0,0.093,0,1.74,KEES,0.536,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.281,1.573
48" x 6",0.734,0.306,http://www.kees.com/pdf/pdssdl.pdf,15,Stainless Steel,0,0.093,0,4.24,KEES,0.536,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.281,4.073
70" x15",1.417,0.683,http://www.kees.com/pdf/pdssdl.pdf,13,Stainless Steel,0,0.277,0,6.073,KEES,1.271,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.818,5.906
9" x 6",0.734,0.306,http://www.kees.com/pdf/pdssdl.pdf,2,Stainless Steel,0,0.093,0,0.974,KEES,0.536,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.281,0.823
60" x12",1.161,0.506,http://www.kees.com/pdf/pdssdl.pdf,11,Stainless Steel,0,0.233,0,5.24,KEES,1.016,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.573,5.073
40" x10",0.995,0.511,http://www.kees.com/pdf/pdssdl.pdf,7,Stainless Steel,0,0.183,0,3.573,KEES,0.849,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.49,3.406
35" x15",1.417,0.683,http://www.kees.com/pdf/pdssdl.pdf,6,Stainless Steel,0,0.277,0,3.156,KEES,1.271,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.818,2.99
36" x 6",0.734,0.306,http://www.kees.com/pdf/pdssdl.pdf,11,Stainless Steel,0,0.093,0,3.24,KEES,0.536,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.281,3.073
50" x15",1.417,0.683,http://www.kees.com/pdf/pdssdl.pdf,9,Stainless Steel,0,0.277,0,4.406,KEES,1.271,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.818,4.24
70" x12",1.161,0.506,http://www.kees.com/pdf/pdssdl.pdf,13,Stainless Steel,0,0.233,0,6.073,KEES,1.016,D3040100,http://www.kees.com/pdf/isdssdl0413.pdf,0,www. BIMConsultingServices.net,0.573,5.906
